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2nd June 2023
Haringey Council London Borough

Planning, Regeneration & Economy

Level 6, River Park House

225 High Road

Wood Green

N22 8HQ
Dear Team,

SITE:  PIZZA EXPRESS, 30 HIGHGATE HIGH STREET, LONDON, N6 5JG
DESIGN AND ACCESS STATEMENT
Use

Restaurant 

Amount 

Not applicable.  Our application is for signage / advertisements and the painting of the building, and we are proposing no other works to the building. 
Layout

Please refer to drawing nos: 596761-1,2,3,4 & 5. Please also refer to visual PX Highgate Rev C.
Scale

Not applicable.  Our application relates only to the installation of signage / adverts and the painting of the window frames and door and on an existing building.  We are not proposing any new buildings as part of this application.

Landscaping

Not applicable.  Our application relates only to the installation of signage / adverts and the painting of the window frames and door on an existing building.  No new landscaping is to take place or any existing landscaping impacted upon as part of this application.

Appearance

Please refer to drawing nos. nos: 596217-1,2,3,4 & 5.  Please refer to Visual PX Derby Iron Gate Rev E.

2 SETS OF EXTERNALLY ILLUMINATED FASCIA TEXT – To replace existing. Folded and welded 2.5mm ali fascia panel is finished satin black.  Flat cut 10mm black acrylic PIZZERIA letters have 1.5mm ali faces covered with gold leaf.  Backs are fixed to the fascia panel on black locators.  Externally illuminated by warm white LEDs which are fitted within a recessed lightline.
2 NON ILLUMINATED AWNINGS – To replace existing.  Orange-brown awnings with log in black and text in black.  
1 EXTERNALLY ILLUMINATED PROJECTION SIGN  - To replace existing.  Flat cut 8mm ali hanging panel is finished black.  Logo is an Ivory RAL 1015 vinyl disc applied to the faces with the graphics and text in black.  Black steel projection arm is fitted with black steel troughs.  Troughs fitted with low energy warm white LEDS for external illumination.

INTERNALLY ILLUMINATED DELIVERY SIGN – To replace take away sign.  1.2mm descaled stainless steel front rim, back and return are finished satin black and are fixed around a steel inner frame.  5mm clear acrylic face is reverse decorated with black opaque vinyl and translucent magenta RAL 4010 text.  Letters are internally illuminated by low energy cool white LEDS. Sign is hung behind the glazing on steel wires which fix to the ceiling.

INTERNALLY ILLUMINATED ROUNDEL  - Roundel is a hollowed ut face of 30mm opal 1T77 perspex which has the sides painted opaque black.  Opal acrylic is fixed over a flat 2.5mm black ali back which is screw fixed to black 25x25 SHS rails.  Fitted with low energy warm white LEDs for face illumination.  Fixed behind the glazing with the rails fixed to the ceiling above and to the floor below.

PAINTING OF FACE – In Farrow & Ball Railings. Fascia to be painted black.
Our design team has looked at all aspects of upgrading the signage at this site and has always been aware to produce a design concept that compliments the listed building and surrounding area.  We feel the subtle change in the signage and painting of the façade will have no detrimental impact on the building and surrounding units.  All existing fixtures and fittings where possible will be used.
Access

Not applicable. Our application relates to signage / adverts only and the painting of the façade.   There will be no change to the current access arrangements as part of this application.
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