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4 June 2026

Planning Condition Discharge 
HGY/2025/0818 Tottenham Hale Station

Dear Planning Team, 

As per the planning approval granted on 30th June 2025 this letter lays out our discharge of conditions 1 and 18.

Condition 1
The development hereby authorised shall be carried out in accordance with the following approved plans, save for any changes which form the final worked up and detailed implementable scheme which shall be submitted to and approved in writing by the Local Planning Authority prior to commencement of development. These changes shall have been co-designed with local stakeholders, including Disability Action Haringey, which shall be clearly evidenced in the submission, and the development shall be carried out in accordance with those details:

Attached with this letter are the following finalised general arrangement drawings:
· General Arrangement (1of 3)
· General Arrangement (2 of 3)
· General Arrangement (3 of 3)

The updates from planning are:
· Station Crossing (Western): We have moved to a single stage, straight through crossing. This removes the stagger and provides a much more direct and accessible route – developed through engagement with Haringey Cycle Champaign. We have included an all round pedestrian phase on all crossings which is an addition to the current layout.
· Eastern Crossing Island: We have increased the pedestrian refuge island width from 1.0m to 1.5m to provide better protection and space.
· Floating Bus Stop: We are ensuring the bus flag is positioned at the front door of the stop to assist visually impaired users. We are also ensuring the shelter and flag locations are aligned correctly with a 2m offset. We have assessed the floating bus stop against the newly released DfT guidance (ATE: Floating bus stops provision and design (Published 26 January 2026) and the bus-stop is compliant (see table 1 below).
· Reduced Street Clutter: By simplifying the signal design and removing unnecessary internal stop lines, we are reducing the number of signal poles on the footway.
· CCTV and Bollards The locations of the CCTV and relocated bollards are indicated on the plans. 

	Design details
	Optimum values

	Island width
	3.5m desired; 2.5m minimum (contextual justification required if otherwise, see process steps)
PROPOSED ISLAND WIDTH IS 2.75m

	Footway width
	2m desired; 1.5m minimum
PROPOSED FOOTWAY WIDTH AT REAR OF ISLAND VARIES 2.3m to 2.5m TO BACK OF HIGHWAY 

	Cycle track width 1 way
	2m desired, 1.5m minimum
1 WAY BYPASS CYCLE TRACK IS 1.6m

	Cycle track width 2 way
	3m desired; 2.5m minimum
N/A

	Crossing type
	Zebra
PROVIDED

	Shelter position
	On island
PROVIDED

	Level difference from cycle track to footway
	125mm desired; 50mm minimum 50mm 
LEVEL DIFFERENCE PROVIDED

	Material visual contrast between cycle track and footway
	High (see Inclusive mobility)
PROVIDED:
ASPHALT CYCLE TRACK & CONCRETE PAVED FOOTWAY/ISLAND DELINEATED WITH GRANITE EDGE/KERB

	Tactile paving
	Red blister with controlled crossing
PROVIDED

	Forward visibility for cyclists
	See LTN 1/20 table 5.5
FORWARD VISIBILITY OF 31m ACHIEVED. (REQUIRED FOR CYCLIST TRAVELLING AT 30kph)

	Measures to slow cyclists
	Horizontal and vertical deflection; signing and markings
HORIZTONAL AND VERTICAL DEFLECTION PROVIDED (Ramps & Markings at Crossing) 


Table 1 showing compliance with DfT guidance on floating bus stops


As per Condition 1 the above changes have been presented and discussed with key stakeholders including, MET Designing out Crime officer, Haringey Cycling Champaign and Haringey Disability Action.

There was support for these changes (see appendix 1). Although DAH continue to object to the principle of a floating bus stop.  An Equality Impact Assessment has been undertaken on the scheme and considered this concern as part of our equality duty.

Condition 18
The works, hereby approved, shall include features to reduce crime and
promote a safe environment for the public, details of which shall have been
submitted to and approved in writing by the Local Planning Authority prior to
first use.

As noted above and on the GAs new lighting and CCTV cameras will be installed.  A meeting was held with the MET Designing out Crime Officers on 17th December 2025 and they confirmed their support for the proposals.

We trust that this provides you with the required information to approve this minor amendment.


Yours sincerely
[image: ]
	

	

	

	Sam Neal
Project manager - major projects team
Highways














Appendix 1 – Stakeholder Feedback on design changes post planning

24 February 2026

Thanks so much for this - looks like a big improvement on design Michael had talked to me before about. I'm still not sure how folks cycling towards Walthamstow arriving on the bidirectional on Broad Lane don't cause pedestrian conflict? As in they'll go to toucan, cross turning right and then be on crossing with pedestrians? But overall seems fairly decent - much thanks.
 
---
Simon Munk (he/him)
Head of Campaigns & Community Development
London Cycling Champaign

-------------------------------------------------------------------------------------------------------------------------------------------

24 February 2026

Many thanks Sam,
 
The new crossing layout is a big improvement.  As Simon observes, there’s still some conflict built in, but it should be minimised by the generous width. 
 
Best regards,
 
Michael Poteliakhoff
Consultations Coordinator Haringey Cycle Campaign

------------------------------------------------------------------------------------------------------------------------------------------
Meeting Notes Disability Action Haringey – 20 February 2026
 
Please see below a short summary of our meeting, please let me know if I have missed anything.
 
1. We took you through the revised general arrangement drawing highlighting the key changes since the planning submission as per the below:
Station Crossing (Western): We have moved to a single stage, straight through crossing. This removes the stagger and provides a much more direct and accessible route. Also we will have an all-round pedestrian phase on all crossings (currently it is not).
Eastern Crossing Island: We have increased the pedestrian refuge island width from 1.0m to 1.5m to provide better protection and space.
Floating Bus Stop: We are ensuring the bus flag is positioned at the front door of the stop to assist visually impaired users. We are also ensuring the shelter and flag locations are aligned correctly with a 2m offset. The scheme is compliant with the new DfT guidance 
Reduced Street Clutter: By simplifying the signal design and removing unnecessary internal stop lines, we are reducing the number of signal poles on the footway.
CCTV and Bollards The locations of the CCTV have been finalised
 
2. We highlighted our review of the floating bus stop design against the newly released ATE: Floating bus stops provision and design (Published 26 January 2026) 
 
3. Elements raised in the discussion
· Concern regarding the trees around the floating bus stop limiting visibility – these are existing mature trees so we will not be able to remove or relocate.  We will however ensure that the canopy of the trees is at lease a height of 2m to ensure visibility
· Straight through crossing welcomed but may pose an issue for those with slower mobility – it was noted that the other pedestrian crossing to the East of the bus station junction provided a shorter crossing point. 
· It was noted by DAH that cycling is a significant mode of mobility for the disabled community but vast majority of DAH community think mixed use (cycling/ pedestrians) is a risk
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