Mallinson Centre, Highgate School, Bishopswood Road N6 4NY
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	Tree ID
	Common Name
	Height (m)
	DBH (mm)
	Crown spread (m)
	Age Class
	Physiological Condition
	Structural Condition
	Observations
	Recommendation
	Priority
	Insp Freq


	3660
	Common Lime
	20
	800
	8
	M
	Good
	Good
	Tall tree with extending limbs. Significant dead wood over road.
	Remove significant dead wood. Reduce canopy by 5m to reduce risk of failure

	6 
	12 

	3661
	Common Lime x 4
	15
	600
	10
	M
	Good
	Good
	Line of 4 lime trees. Long limbs extending over road and parked cars. Dead wood.
	Reduce overextending limbs by 2-3m to reduce risk of failure. Remove significant dead wood.

	6 
	12

	3662
	Common Lime
	25
	800
	13
	M
	Good
	Good
	Tall tree with long extending limbs.
	Reduce canopy by 5m to reduce risk of failure.

	6 
	12

	3663
	Common Lime
	25
	600
	13
	M
	Good
	Good
	Tall tree with long extending limbs.
	Reduce canopy by 5m to reduce risk of failure.

	6
	12

	3664
	Common Lime
	25
	800
	8
	M
	Good
	Good
	Tall tree next to road.
	Reduce canopy by 5m to reduce risk of failure.

	6
	12

	3665
	Sycamore
	9
	1100
	6
	OM
	Good
	Poor
	Kretzschmaria fruiting bodies on tension side at base and up stem. Root girdling, dysfunction and decay at base.

	Fell.
	6
	12

	3669
	Sycamore
	18
	300
	5
	OM
	Poor
	Fair
	2x dying trees. It is possible that nitrogen leaching from the grass clipping pile up hill is contributing to the significant number of dying trees.

	Fell 
	6
	12

	3670
	Sycamore
	17
	500
	5
	OM
	Poor
	Fair
	Dying tree.
	Fell.
	6 
	12

	3671
	Sycamore
	18
	300
	4
	OM
	Poor
	Fair
	Dying tree.
	Fell.
	6
	12

	3672
	Dead tree
	3
	150
	2
	D
	Dead
	Fair
	Dead tree.
	Fell.
	6 
	12

	3675
	Sycamore
	10
	150
	3
	M
	Good
	Fair
	Regrowth from stump.
	Fell.
	6
	12

	3676
	Common Ash
	18
	500
	6
	M
	Fair
	Good
	Significant dead wood throughout canopy.
	Remove significant dead wood.

	6
	12 

	3679
	Sycamore
	18
	800
	10
	M
	Good
	Good
	Extended limb over road.
	Reduce extended limb by 3m.

	6
	12

	3680
	Common Lime
	18
	700
	10
	M
	Good
	Good
	Dead wood over footpath.
	Reduce canopy by 5m to reduce risk of failure. Remove significant dead wood.

	6 
	12
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