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www.londonsash.com
Replacement Double Glazed Sashes
Replacement Sashes
• Removal of old sashes and legal disposal
• New made to measure sashes made from Grade-A Redwood*
• All profile details as per historic originals including mouldings, glazing bars & horns.
• ‘Applied bar’ construction
• Double glazing: Softcoat double glazing with a U-Value from 1.1w/m2K
• Primer and undercoat applied
• Painted in 2-further coats of white microporous paint**
• Windows fitted with draught proof beading.
• New cords & weights
Frame Decoration 
• Boxes and frames cleaned of debris
• Coat of primer undercoat applied where required
(Further decoration may be required at your own cost)
Window furniture
• Fitted in polished brass***
• 1x Brighton window fastener
• 2x Sash finger lifts
• 2x Exterior D-handles
• 2x Key operated dual position security locks
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