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Air Quality and Dust Management Plan (AQDMP)
In accordance with Greater London Authority SPG Dust and Emissions Control (2014)
Site Address
37–39 West Road, London, N17 0RE

1. Introduction
This Air Quality and Dust Management Plan (AQDMP) has been prepared to ensure that all demolition and construction activities undertaken by BibbEgan at 37–39 West Road, London, N17 0RE are carried out in a manner that minimises impacts on air quality and the surrounding environment.
This AQDMP has been prepared in accordance with the requirements of the Planning Sub-Committee and associated planning conditions.
This plan is informed by BibbEgan’s Environmental Policy (January 2026) and reflects the company’s commitment to preventing pollution, reducing emissions, and protecting local communities.

2. Mitigation Measures to Control Dust Emissions
In accordance with company policy and best practice, the following mitigation measures will be implemented:
General Site Controls
· Maintain high standards of housekeeping across all work areas
· Enclose or screen working areas where practicable
· Use water suppression (e.g. damping down) during dust-generating activities
· Employ vacuum extraction or filtered systems on static plant where possible
· Use sheeting or barriers to prevent dust migration beyond site boundaries
During Demolition and Construction Activities
· Damping down of stockpiles and exposed materials
· Use of water sprays during cutting, crushing, and loading operations
· Avoid dry sweeping; use wet cleaning or vacuum systems
· Minimise drop heights during material handling
· Sequence works to reduce dust generation

Vehicle and Transport Controls
· All wagons and skips to be covered when leaving site
· Wheel washing facilities to be used where necessary
· Site access routes to be kept clean and damped down
· Engines switched off when not in use (anti-idling policy)

Monitoring and Community Protection
· Regular visual inspections for dust emissions
· Immediate corrective actions where dust is observed
· Works planned to minimise nuisance to local residents
· Complaints procedure in place with rapid response


3. NRMM Registration (Non-Road Mobile Machinery)
· The site at 37–39 West Road, London, N17 0RE will be registered on the NRMM London Register prior to commencement of works: http://nrmm.london
· All applicable plant will comply with current emissions standards as required by GLA guidance
· Evidence of registration will be maintained and made available on site


4. NRMM Compliance and Documentation
In line with BibbEgan’s Environmental Policy:
· All NRMM and plant will:
· Meet required EU Stage emission standards
· Be regularly serviced and maintained
· Operate efficiently to minimise emissions
· The following documentation will be kept on site:
· NRMM registration confirmation
· Engine emission compliance certificates
· Maintenance and servicing logs
· Plant inspection records
· Documentation will be made available at all times for Local Authority inspection

5. Inventory of NRMM on Site
An up-to-date inventory of all Non-Road Mobile Machinery will be maintained on site, including:
· Plant type and description
· Manufacturer and model
· Engine emission stage (e.g. Stage IV / Stage V)
· Unique identification / registration number
· Date of last service and maintenance records
This inventory will be:
· Reviewed regularly
· Updated when plant is added or removed
· Available for inspection at all times


6. Dust Risk Assessment
A project-specific Dust Risk Assessment has been considered for works at 37–39 West Road, London, N17 0RE, taking into account:


Key Risk Factors
· Nature and scale of demolition and construction activities
· Proximity to sensitive receptors including residential properties and local businesses
· Site layout and prevailing weather conditions
· Duration of dust-generating activities

Risk Classification
The works are anticipated to present a Medium Risk of dust generation in accordance with GLA guidance due to the nature of demolition activities and proximity to surrounding receptors.
Control Measures
· Standard and enhanced mitigation measures outlined in Section 2 will be implemented
· Additional controls will be introduced where necessary based on ongoing site conditions
· Continuous monitoring and review will be undertaken throughout the project

7. Lorry Management and Parking Arrangements
· Lorry movements will be planned and coordinated to minimise disruption and emissions
· Where appropriate, joint lorry holding areas or consolidation arrangements will be utilised
· No unnecessary idling of vehicles will be permitted
· Delivery schedules will be managed to avoid peak congestion periods
· All drivers will be briefed on site environmental controls

8. Monitoring, Compliance and Review
· Regular environmental inspections will be carried out by Site Management
· Dust control measures will be reviewed and adjusted as required
· Records of inspections, monitoring, and corrective actions will be maintained
· The AQDMP will be reviewed:
· Periodically during the project
· Following any complaints or incidents
· If site conditions or scope of works change


9. Responsibilities
· Managing Director (James Bibbey): Overall responsibility for environmental compliance
· Project Managers: Implementation and monitoring of AQDMP
· Site Supervisors: Day-to-day enforcement of dust control measures
· Employees and Subcontractors: Compliance with site procedures and reporting of issues
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