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	Our ref: HGY/2026/0937
Contact: Ben Coffie

Date: 09/06/2026

	Town and Country Act 1990 (As amended)

	Location:
	88 St Pauls Road, Tottenham, London, N17 0NE

	Proposal:
	Approval of details reserved by conditions 3 (external materials), 4 (hard and soft landscape), 6 (Energy Statement) attached to planning permission with ref: HGY/2025/1956 for the demolition of an existing commercial unit and conversion of the remaining commercial unit into a 1b|1p dwelling with associated access and landscaping.

	Wording of condition 6:
	The development hereby approved shall be constructed in accordance with
the Energy statement by T16 Design (dated October, 2025) delivering a minimum 39% improvement on carbon emissions over 2021 Building Regulations Part L, with high fabric efficiencies, air source heat pumps (ASHPs).

(a) Prior to above ground construction, details of the Energy Strategy shall
be submitted to and approved by the Local Planning Authority. This must
include:

· Details of the PV, demonstrating the roof area has been maximised,
with the following details: a roof plan; the number, angle, orientation, type,
and efficiency level of the PVs; how overheating of the panels will be
minimised; their peak output (kWp); inverter capacity; and how the energy
will be used on-site before exporting to the grid;

The development shall be carried out strictly in accordance with the details
so approved prior to first operation and shall be maintained and retained for
the lifetime of the development.

(b) The solar PV arrays must be installed and brought into use prior to first
occupation of the relevant block. Six months following the first occupation of
that block, evidence that the solar PV arrays have been installed correctly
and are operational shall be submitted to and approved by the Local
Planning Authority, including photographs of the solar array, installer confirmation, an energy generation statement for the period that the solar PV array has been installed, and a Microgeneration Certification Scheme certificate. The solar PV array shall be installed with monitoring equipment prior to completion and shall be maintained at least annually thereafter.

Reason: To ensure the development reduces its impact on climate change
by reducing carbon emissions on site in compliance with the Energy Hierarchy, and in line with London Plan (2021) Policy SI2, and Local Plan (2017) Policies SP4 and DM22.



Carbon Management Response 24/04/2026

Documents submitted:
· Proposed roof plan showing PV layout 
· PV specification (Chelsfield solar)
· PV specification (Installation details) 

Response
The current PV system has been proposed to achieve 4.5kWp output with 10 number of PV panels (@450W). 

Actions: 
· Applicant should submit the details of the Energy Strategy, this should demonstrate the minimum percentage of the carbon emissions has been achieved and ASHP system have been proposed as per the wording of the planning condition. 
· Applicant should note the part (b) requirement of the planning condition. They should ensure the solar PV array to be installed under Microgeneration Certification scheme. 

Conclusion
Further information is required so we therefore do not recommend discharging Condition 6(a). The applicant should provide a response to the points raised above and issue updated plans/information where required.


Carbon Management Response 09/06/2026

Documents submitted:
· 6703 - Energy Statement for planning - Rev 6 - Issued 04.06.2026

Response
The submitted Energy Statement has provided following the carbon reductions of the current proposal: 

	Residential 
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	Total regulated emissions 
(Tonnes CO2 / year) 
	CO2 savings
(Tonnes CO2 / year) 
	Percentage savings
(%)

	Part L 2021 baseline 
	0.6
	
	

	Be Lean 
	0.5
	-
	22%

	Be Clean 
	0.5
	-
	0%

	Be Green 
	-0.0011
	-
	80%

	Cumulative savings
	
	0.6011
	102%

	Carbon shortfall to offset (tCO2)
	0
	
	

	Carbon offset contribution
	£95 x 30 years x 0tCO2/year = £0



The submitted ES has confirmed Air Source Heat Pumps and 8 number of 0.45kWp PV panels (with a total output of 4.6 kWp) have been proposed for the development. 

Conclusion
The submitted information is acceptable and we can recommend that Condition 6 is discharged.

