FIRE SAFETY STRATEGY REPORT
79 WESTBEECH ROAD
LONDON
N22 6HU


1.Introduction

This fire safety strategy outlines the measures required to comply with 
Part B of the Building Regulations in relation to a single storey rear extension of a terrace single-family dwelling.
The purpose is to ensure safe means of escape, containment of fire, and early warning system.


2.Building Description

Type: Terrace single-family dwelling
Number of Storeys (existing):  2
Use Class: D3 (Dwelling House)
Purpose: Habitable rooms
Construction Type: 
Traditional brick with timber and flat roof.


3.Means of Escape:

3.1 Provided a protected hallway opening onto the escape route on the ground floor.

3.2 Escape Window:
Escape windows to first floor rooms to be provided for additional safety.


4. Fire Detection and Alarm System:
A Grade D1 LD2 fire detection system will be installed.
Mains-powered smoke alarms with battery backup on each storey landing level and heat alarm in the kitchen.
All alarms will be interlinked and installed accordance with BS 5839-6: 2019


5. Fire Compartmentation:

Walls and roof will have adequate resistance to prevent vertical and horizontal fire spread (one hour fire protection).




6.Access and Firefighting

As a domestic dwelling, direct access from the street for fire and rescue services is sufficient. Firefighting access remains unchanged post- extension.


7.Materials and Construction:

All materials used must meet reaction to fire [performance standards as per Approved Document Part B.


8.Conclusion: 

This fire safety strategy ensures the proposed rear extension complies with relevant fire safety requirements, ensuring life safety and regulatory compliance.
Implementation must be verified on-site and signed off by Building Control.





