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®

Fibre Initial Site Checklist 
NSI: L/BOW/00X            Site Name: Chocolate Factory Project Date: 27/10/22
Developer: Formations


Site Project Manager: Mark O'Dwyer
Contact Number: 07752029429
E Mail: mark.odwyer@formationgroupplc.com
This form is to be discussed, agreed, and signed by both parties.
Confirm the Site Proposals are acceptable
 Check from where developer can provide a duct and cable route into site for the build programme.
Explain there will be charges for re-plans if the developer’s layout changes. Emphasise the point that with fibre this is much more complex to do. 
Determine any requirements for site copper landlord service lines eg Lifts / Alarms / BMS / CCTV / EV Charging / Pumps. No copper lines allowed for residential plots on a fibre site and these addresses are postcode block for copper service. 
Seek to secure the Council Addressing for the site at the earliest opportunity
Discuss the developers’ responsibilities for quality of work on site and provision of plant, to facilitate cabling and jointing work. Outline the importance of completing work correctly first time to avoid remedial work. That all duct blockages that prevent Openreach® connecting the properties will incur a charge to the developer, or these will be cleared by the developer.
Explain the importance of plot management and the need for the Site Manager to inform the NSR of site progresses and plot readiness ensuring that all the work is complete to provide service prior to the property being occupied. Explain also, that Openreach® will seek to recover any payments made to its suppliers for abortive visits to sites where plots have been declared ready by the site manager or his staff.
Discuss the Builders Guide pointing out the Specifications for:-https://www.ournetwork.openreach.co.uk/resources/site1/General/Downloads/copper_developer_handbook.pdf
a. Laying of Openreach® duct, and Construction of boxes (Minimum depth 750mm for Fibre sites).  Explain the options with Pre-formed chambers https://www.cubis-systems.com/uk/stakkabox-quad-for-openreach/  at their cost.
b. Duct to be cut flush with brickwork keeping them away from the side walls & floors. 
c. Brackets (channel irons) and bearers to be installed in all boxes with Foundation Bolts No2 set in brick-built boxes during building.
d. Box level should be flush with ground level and clear of debris.
e. In an unmade surface or grass surface a joint box frame shall be surrounded with a 100mm wide strip of grade C30 concrete, finished with the frame.
f. If external feed the duct at the House/Unit shall be cut off 1 course of bricks above finished ground level and directly in line under the entry point hole into the dwelling.
g. 50mm duct to be presented to outside walls only and 90mm ducts to be presented internally only in risers/ basements. Ducts must not be taken into living areas of a building.  
Explain NO orders can be made or taken via their service provider until all installation works of our equipment into each plot has been completed and tested unlike copper (240volt supply needed for testing). 
What is the preferred location for the duct entry point at the house end – Internal or external?  Internal is the preferred method.
a. If external feed the duct at the House/Unit shall be cut off 1 course of bricks above finished ground level and directly in line under the entry point hole into the dwelling. The developer will then need to consider that the equipment will need to be positioned at this entry point inside the dwelling.
b. Discuss the equipment we will need to install including the size and location and the need for a double power socket.  This must be permanently live before our equipment can be installed and commissioned.
c. Single dwelling units (SDUs) we require 2m of DSI cable outside plot above duct and 1m at the house end with end stops fitted. 
d. Multi dwelling units (MDUs) - Fibre cabling MUST have a 2n coil in each MDU. Cable protection needed to stop damage by other site workers.
Remind the builder that any changes made to the installation Must be agreed beforehand with the New Site Representative and of their obligations to manage the work carried out on site in accordance with the terms and conditions of the SOD contract. Explain the new payment process that the PO wil be provided at the end of the build unless on large sites part payment is required. Stress that sub standard work will have to be remedied before payment will be authorised by the NSR. Point out that under the terms and conditions payment will only be possible for 1 year following the completion of the civils work.
Explain the stores ordering process.  Explain stores are to be signed for on delivery and kept in a secure area designated for Openreach® stores only.  Emphasise free provision /delivery of stores by Openreach® and stress that the stores are only intended for Openreach® use and any misuse, loss and damage will be thoroughly investigated and could be charged for
Check if there is any existing Openreach® plant on site that is still in use. If this requires moving explain this work may be chargeable. For Identification of existing plant and Diversions (Dial 08009173993 for dial before you dig)
Check if any network will cross a third parties land, if it does gather contact details and if possible, gain an agreement.
Ask the developer for details of any 3rd party PIA agreed service providers using the Openreach® plant into site.
Ask the developer for details of their requirements for method statements, risk assessments and site inductions.  
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A copy should be left on site and a copy kept by the NSR
Remember - Please do not abuse a New Site Rep  
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